11.5 Dial-up
Prev | Chapter 11 Web Interface | Next

## 11.5 Dial-up

Users allowed to dial RAS connections (see chapter 15.1 Viewing and definitions of user accounts) can dial and hang up individual RAS links and view their status on the Dial-up lines tab. This tab lists all dial-up lines defined in WinRoute regardless of groups where they belong (for details, see chapter 5 Network interfaces).

Figure 11.12. Web interface — dial-ups control

The following information items are provided for each line:

- RAS interface — name of the interface in WinRoute (see chapter 5 Network interfaces).

- Current state — Disconnected, Connecting, Connected, Disconnecting.

- Action — hypertext link that dials or hangs up the line when clicked (depending on its current state).

- Connection time.

- Volume of data transferred in either direction (Incoming = from the Internet to the LAN, Outgoing = from the LAN to the Internet).

Note: The Dial-up page is automatically refreshed in regular time intervals.

Prev | Up | Next
11.4 User preferences | Contents | Chapter 12 HTTP and FTP filtering