2.3 System requirements
Prev | Chapter 2 Introduction | Next

## 2.3 System requirements

Requirements on minimal hardware parameters of the host where WinRoute will be installed:

- CPU 1 GHz,

- 1 GB RAM,

- Two network interfaces (including dial-ups).

For Windows:

- 50 MB free disk space for installation of Kerio WinRoute Firewall.

- Disk space for statistics (see chapter 21 Kerio StaR - statistics and reporting) and logs (in accordance with traffic flow and logging level — see chapter 22 Logs).

- to keep the installed product (especially its configuration files) as secure as possible, it is recommended to use the NTFS file system.

For Kerio WinRoute Firewall Software Appliance:

- Minimum 3 GB hard disk.

- No operating system is required to be installed on the computer. Any existing operating system will be removed from the computer.

For Kerio WinRoute Firewall VMware Virtual Appliance:

- VMware Player, VMware Workstation or VMware Server.

- 3 GB free disk space.

The following browsers can be used to access the WinRoute (Kerio StaR — see chapter 21 Kerio StaR - statistics and reporting and Kerio SSL-VPN — see chapter 24 Kerio Clientless SSL-VPN (Windows)) web services:

- Internet Explorer 7 or higher,

- Firefox 2 or higher,

- Safari 3 or higher.

Prev | Up | Next
2.2 Conflicting software | Contents | 2.4 Installation - Windows